{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Routing"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Routing","index":0,"n_rows":75,"n_cols":37,"rows_kept":75,"cut":false,"hidden":false,"merged":[[20,31,20,32],[36,9,36,10],[44,18,44,19],[63,26,63,29],[64,26,64,29],[23,28,23,29],[30,27,30,29],[39,24,40,25],[62,26,62,29],[47,11,47,14],[50,11,50,14],[46,11,46,14],[2,32,2,33],[10,30,10,34],[11,30,11,34],[15,24,15,26],[15,31,17,32],[14,23,14,24],[16,25,18,26],[5,34,5,35],[14,26,14,27],[10,25,10,26],[13,26,13,27],[6,35,6,36],[41,34,41,36],[66,34,66,37],[66,23,66,25],[63,30,63,31],[63,23,63,25],[66,27,66,28],[62,20,62,25],[58,22,58,23],[46,33,47,34],[16,2,17,3],[6,17,6,18],[52,18,52,19],[29,12,29,13],[18,19,21,20],[38,19,38,20],[5,20,6,21],[8,20,8,23],[5,23,5,25],[47,5,47,7],[19,28,19,29],[58,24,58,30],[48,24,48,29],[73,23,73,25],[74,23,74,25],[71,30,71,31],[72,30,72,31],[73,30,73,31],[74,30,74,31],[70,23,70,25],[71,23,71,25],[72,23,72,25],[68,23,68,25],[69,23,69,25],[62,30,62,31],[70,30,70,31],[68,27,68,28],[64,4,64,5],[73,27,73,28],[74,27,74,28],[70,27,70,28],[71,27,71,28],[72,27,72,28],[67,23,67,25],[65,23,65,25],[64,23,64,25],[67,27,67,28]]}
[]
[null,"CAUTION!  BEFORE engaging inputs on the 802:"]
[null,"Pad 7/8 on the mixer to prevent serious feedback",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"                                       And Low Voltage Mapping",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"192.168.1.1"]
[null,"Turn the gain on the Presonus Master down"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Speaker Level"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Speaker Level",null,null,"Speakers - Active",null,null,null,null,null,null,null,null,null,null,"FIREWALL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"192.168.2.1"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Monitors - flat reponse active"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PS 2 Mouse ONLY!",null,null,null,null,"ETHERNNET   LAN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"To TCP / IP Network"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"         KVM Mouse"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"!! DO NOT USE USB MOUSE !!"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Speakers - Passive",null,null,null,null,null,null,"SPARE CONNECTIONS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPARE CONNECTIONS",null,null,null,null," "]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"192.168.2.17"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"192.168.2.20"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCOTT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rm 1 - 3"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rm 4 -6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCOTT"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Key Dongle"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"    Aux Input",null,null,null,null,null,"Patch Bay Operation:"]
[null,null,null,null,null,"As needed",null,null,null,null,null,null,"Front              Rear"]
[]
[null,null,null,"  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Continuous Ink Supply"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CD PLAYER"]
[null,null,null,null,null,null,null,null,null,null,null,"Pass Through: "]
[null,null,null,null,null,null,"Hossa Snakes",null,null,null,null,"front and rear top                    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"From Effects"]
[null,null,null,null,null,null,null,null,null,null,null," Rear bottom Rear top              !",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"or  Aux"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"      G y    Y   O    Gn  Bl    V    R      Br",null,null,null,null,null,null,null,"Mixer 2 "]
[null,null,null,null,null,null,null,null,null,null,null,"Cut Off: "]
[null,null,null,null,null,null,null,null,null,null,null,"Insert Top Rear front Bottom"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hossa Snake"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"       Inst. In",null,null,null,null,null,null,null,null,"PHONES 1","PHONES 2"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEGEND",null,null,null,null,null,"COMMENTS",null,null,null,"STATS",null,"IN","OUT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gy","Grey",null,"Mic Level (-60)",null,null,"Studio level is +4 db",null,null,null,"M-AUDIO I / O",null,null,"+ 4"]
[null,null,null,null,"       BASS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gn","Green",null,"Signal Level -10 or +4",null,null,"Home Studio level is -10 db",null,null,null,"MRS 802",null,"+_4","- 10"]
[null,null,null,null,null,"  L    R",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O","Orange",null,"Snake - Signal Level",null,null,null,null,null,null,"ZOOM G2.1",null,"- 20","+ 5"]
[null,null,null,null,null,"KEYBOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bl","Blue",null,"Snake - Instrument Level",null,null,"Created:","2008-03-08",null,null,"24/96 Audio   **",null,"+2","+ 2","**  Consumer-Delta Mixer Default"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Br","Brown",null,"Speaker Level",null,null,"Rev:","2009-07-27",null,null,"24/96 Audio",null,"- 4","+ 2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bk","Black",null,"Computer Cables",null,null,"Rev:3","2010-01-02",null,null,"1622FX",null,"+12@+10","+4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y","Yellow",null,"USB Level Signal (+5 V)",null,null,"Rev 4","December 11,2010",null,null,"Monitors",null,"+ 4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V","Violet",null,"Firewire Level (+5V)",null,null,"Rev 5","2012-08-07",null,null,"Omega"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R","Red",null,"Midi Level Signal",null,null,"Rev 6","2012-09-29",null,null,"ART Pre Amp",null,"+19","-10, +4"]
[null,null,null,null,null,"GUITAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W","White",null,"Cat 5 Ethernet",null,null,"Rev 7","2013-08-23"]
[null,null,null,null,null,null,null,null,null,null,null,"CHANNEL 1",null,null,"CHANNEL 2",null,null,null,null,null,"Rt","Right"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lt","Left"]