[RTClib](http://github.com/adafruit/RTClib) - a library for getting and setting time from a DS1307 (originally written by JeeLab, our version is slightly different so please **only use ours** to make sure its compatible!) - download the .zip by clicking on **Download Source** (top right) and rename the uncompressed folder RTClib